This monitors the round trip network response time from the controller to the agent, and if it goes above a threshold repeatedly, it disconnects the agent.

This is useful for detecting unresponsive agents, or other network problems that clog the communication channel. More specifically, the controller sends a no-op command to the agent, and checks the time it takes to get back the result of this no-op command.